InertiaSDK

Loading...
Searching...
No Matches
Public Member Functions | Public Attributes | List of all members
inertia::FirmwareSettings Struct Reference

Firmware Update Settings. More...

`#include <FirmwareSettings.h>`

## Public Member Functions
| FirmwareSettings ()

## Public Attributes
bool | resetToDefaults
| Reset the device to default settings when reprogramming with new firmware.
std::wstring | firmwareFile
| The Firmware Update file.
bool | validateHardwareID
| Validate if FWU target hardware ID and device hardware ID match.
bool | validateHardwareRevision
| Validate if FWU target firmware ID and device firmware ID match.
bool | validateFirmwareID
| Validate if FWU target hardware revision and device hardware revision match.
bool | validateFirmwareComponent
| Validate if the device supports the selected FWU target components.
std::vector< unsigned > | indexes
| The indexes of the target components in the FWU file that should be reprogrammed, empty for all. Order does not matter, the lowest index is always updated first.

## Detailed Description

Firmware Update Settings.

Class containing settings for Firmware Validation and Reprogramming.

## Constructor & Destructor Documentation

## ◆ FirmwareSettings()

inertia::FirmwareSettings::FirmwareSettings | ( |  | ) |

Default constructor.

The documentation for this struct was generated from the following file:

- FirmwareSettings.h